

#HW-1,4110056009陳柏硯

(1)allocate\_map()




(2)allocate\_pid

一般Allocate





Full of bit map



(3) release\_pid()

If PID is not allocated



(4)exit

(5)out of choice

